#MicroXplorer Configuration settings - do not modify
BOOTPATH.BootPathName=LEGACY
BOOTPATH.IPParameters=BootPathName
BOOTPATH.UserSelectedBootPath=LEGACY
CAD.formats=[]
CAD.pinconfig=Dual
CAD.provider=Component Search Engine
CORTEX_M33_NS.userName=CORTEX_M33
File.Version=6
GPDMA1.CIRCULARMODE_GPDMACH1=ENABLE
GPDMA1.CIRCULARMODE_GPDMACH3=ENABLE
GPDMA1.DESTINC_GPDMACH1=DMA_DINC_INCREMENTED
GPDMA1.DESTINC_GPDMACH3=DMA_DINC_INCREMENTED
GPDMA1.DIRECTION_GPDMACH0=DMA_MEMORY_TO_PERIPH
GPDMA1.DIRECTION_GPDMACH2=DMA_MEMORY_TO_PERIPH
GPDMA1.IPHANDLE_GPDMACH0-SIMPLEREQUEST_GPDMACH0=__NULL
GPDMA1.IPHANDLE_GPDMACH1-SIMPLEREQUEST_GPDMACH1=__NULL
GPDMA1.IPHANDLE_GPDMACH2-SIMPLEREQUEST_GPDMACH2=__NULL
GPDMA1.IPHANDLE_GPDMACH3-SIMPLEREQUEST_GPDMACH3=__NULL
GPDMA1.IPParameters=REQUEST_GPDMACH0,CIRCULARMODE_GPDMACH1,LINKALLOCATEDPORT_CIRCULAR_GPDMACH1,REQUEST_GPDMACH1,TRANSFERALLOCATEDPORTDEST_GPDMACH1,TRANSFEREVENTMODE_LL_CIRCULAR_GPDMACH1,DIRECTION_GPDMACH0,SRCINC_GPDMACH0,DESTINC_GPDMACH1,TRANSFERALLOCATEDPORTSRC_GPDMACH1,TRANSFERALLOCATEDPORTSRC_GPDMACH0,REQUEST_GPDMACH2,DIRECTION_GPDMACH2,SRCINC_GPDMACH2,TRANSFERALLOCATEDPORTSRC_GPDMACH2,IPHANDLE_GPDMACH2-SIMPLEREQUEST_GPDMACH2,IPHANDLE_GPDMACH1-SIMPLEREQUEST_GPDMACH1,IPHANDLE_GPDMACH0-SIMPLEREQUEST_GPDMACH0,CIRCULARMODE_GPDMACH3,LINKALLOCATEDPORT_CIRCULAR_GPDMACH3,IPHANDLE_GPDMACH3-SIMPLEREQUEST_GPDMACH3,REQUEST_GPDMACH3,DESTINC_GPDMACH3,TRANSFERALLOCATEDPORTDEST_GPDMACH3
GPDMA1.LINKALLOCATEDPORT_CIRCULAR_GPDMACH1=DMA_LINK_ALLOCATED_PORT1
GPDMA1.LINKALLOCATEDPORT_CIRCULAR_GPDMACH3=DMA_LINK_ALLOCATED_PORT1
GPDMA1.REQUEST_GPDMACH0=GPDMA1_REQUEST_USART3_TX
GPDMA1.REQUEST_GPDMACH1=GPDMA1_REQUEST_USART3_RX
GPDMA1.REQUEST_GPDMACH2=GPDMA1_REQUEST_USART2_TX
GPDMA1.REQUEST_GPDMACH3=GPDMA1_REQUEST_USART2_RX
GPDMA1.SRCINC_GPDMACH0=DMA_SINC_INCREMENTED
GPDMA1.SRCINC_GPDMACH2=DMA_SINC_INCREMENTED
GPDMA1.TRANSFERALLOCATEDPORTDEST_GPDMACH1=DMA_DEST_ALLOCATED_PORT1
GPDMA1.TRANSFERALLOCATEDPORTDEST_GPDMACH3=DMA_DEST_ALLOCATED_PORT1
GPDMA1.TRANSFERALLOCATEDPORTSRC_GPDMACH0=DMA_SRC_ALLOCATED_PORT1
GPDMA1.TRANSFERALLOCATEDPORTSRC_GPDMACH1=DMA_SRC_ALLOCATED_PORT0
GPDMA1.TRANSFERALLOCATEDPORTSRC_GPDMACH2=DMA_SRC_ALLOCATED_PORT1
GPDMA1.TRANSFEREVENTMODE_LL_CIRCULAR_GPDMACH1=DMA_TCEM_BLOCK_TRANSFER
GPDMA2.CIRCULARMODE_GPDMACH0=ENABLE
GPDMA2.CIRCULARMODE_GPDMACH1=ENABLE
GPDMA2.CIRCULARMODE_GPDMACH2=ENABLE
GPDMA2.CIRCULARMODE_GPDMACH3=ENABLE
GPDMA2.DESTDATAWIDTH_GPDMACH0=DMA_DEST_DATAWIDTH_WORD
GPDMA2.DESTDATAWIDTH_GPDMACH1=DMA_DEST_DATAWIDTH_WORD
GPDMA2.DESTDATAWIDTH_GPDMACH2=DMA_DEST_DATAWIDTH_WORD
GPDMA2.DESTDATAWIDTH_GPDMACH3=DMA_DEST_DATAWIDTH_WORD
GPDMA2.DESTINC_GPDMACH1=DMA_DINC_INCREMENTED
GPDMA2.DESTINC_GPDMACH3=DMA_DINC_INCREMENTED
GPDMA2.DIRECTION_GPDMACH0=DMA_MEMORY_TO_PERIPH
GPDMA2.DIRECTION_GPDMACH2=DMA_MEMORY_TO_PERIPH
GPDMA2.IPHANDLE_GPDMACH0-SIMPLEREQUEST_GPDMACH0=__NULL
GPDMA2.IPHANDLE_GPDMACH1-SIMPLEREQUEST_GPDMACH1=__NULL
GPDMA2.IPHANDLE_GPDMACH2-SIMPLEREQUEST_GPDMACH2=__NULL
GPDMA2.IPHANDLE_GPDMACH3-SIMPLEREQUEST_GPDMACH3=__NULL
GPDMA2.IPParameters=CIRCULARMODE_GPDMACH0,LINKALLOCATEDPORT_CIRCULAR_GPDMACH0,REQUEST_GPDMACH0,DIRECTION_GPDMACH0,SRCINC_GPDMACH0,SRCDATAWIDTH_GPDMACH0,TRANSFERALLOCATEDPORTSRC_GPDMACH0,DESTDATAWIDTH_GPDMACH0,CIRCULARMODE_GPDMACH1,LINKALLOCATEDPORT_CIRCULAR_GPDMACH1,REQUEST_GPDMACH1,SRCDATAWIDTH_GPDMACH1,DESTDATAWIDTH_GPDMACH1,TRANSFERALLOCATEDPORTDEST_GPDMACH1,DESTINC_GPDMACH1,CIRCULARMODE_GPDMACH2,LINKALLOCATEDPORT_CIRCULAR_GPDMACH2,REQUEST_GPDMACH2,DIRECTION_GPDMACH2,SRCINC_GPDMACH2,SRCDATAWIDTH_GPDMACH2,TRANSFERALLOCATEDPORTSRC_GPDMACH2,DESTDATAWIDTH_GPDMACH2,IPHANDLE_GPDMACH1-SIMPLEREQUEST_GPDMACH1,IPHANDLE_GPDMACH2-SIMPLEREQUEST_GPDMACH2,IPHANDLE_GPDMACH0-SIMPLEREQUEST_GPDMACH0,CIRCULARMODE_GPDMACH3,LINKALLOCATEDPORT_CIRCULAR_GPDMACH3,IPHANDLE_GPDMACH3-SIMPLEREQUEST_GPDMACH3,REQUEST_GPDMACH3,SRCDATAWIDTH_GPDMACH3,DESTINC_GPDMACH3,DESTDATAWIDTH_GPDMACH3,TRANSFERALLOCATEDPORTDEST_GPDMACH3
GPDMA2.LINKALLOCATEDPORT_CIRCULAR_GPDMACH0=DMA_LINK_ALLOCATED_PORT1
GPDMA2.LINKALLOCATEDPORT_CIRCULAR_GPDMACH1=DMA_LINK_ALLOCATED_PORT1
GPDMA2.LINKALLOCATEDPORT_CIRCULAR_GPDMACH2=DMA_LINK_ALLOCATED_PORT1
GPDMA2.LINKALLOCATEDPORT_CIRCULAR_GPDMACH3=DMA_LINK_ALLOCATED_PORT1
GPDMA2.REQUEST_GPDMACH0=GPDMA2_REQUEST_SPI2_TX
GPDMA2.REQUEST_GPDMACH1=GPDMA2_REQUEST_SPI2_RX
GPDMA2.REQUEST_GPDMACH2=GPDMA2_REQUEST_SPI3_TX
GPDMA2.REQUEST_GPDMACH3=GPDMA2_REQUEST_SPI3_RX
GPDMA2.SRCDATAWIDTH_GPDMACH0=DMA_SRC_DATAWIDTH_WORD
GPDMA2.SRCDATAWIDTH_GPDMACH1=DMA_SRC_DATAWIDTH_WORD
GPDMA2.SRCDATAWIDTH_GPDMACH2=DMA_SRC_DATAWIDTH_WORD
GPDMA2.SRCDATAWIDTH_GPDMACH3=DMA_SRC_DATAWIDTH_WORD
GPDMA2.SRCINC_GPDMACH0=DMA_SINC_INCREMENTED
GPDMA2.SRCINC_GPDMACH2=DMA_SINC_INCREMENTED
GPDMA2.TRANSFERALLOCATEDPORTDEST_GPDMACH1=DMA_DEST_ALLOCATED_PORT1
GPDMA2.TRANSFERALLOCATEDPORTDEST_GPDMACH3=DMA_DEST_ALLOCATED_PORT1
GPDMA2.TRANSFERALLOCATEDPORTSRC_GPDMACH0=DMA_SRC_ALLOCATED_PORT1
GPDMA2.TRANSFERALLOCATEDPORTSRC_GPDMACH2=DMA_SRC_ALLOCATED_PORT1
GPIO.groupedBy=Group By Peripherals
I2C1.IPParameters=Timing
I2C1.Timing=0x00707CBB
I2S2.AudioFreq=AudioFreqCustomValue
I2S2.AudioFreqCustom=32000
I2S2.DataFormat=I2S_DATAFORMAT_32B
I2S2.ErrorAudioFreq=0.0 %
I2S2.IPParameters=Instance,RealAudioFreq,ErrorAudioFreq,DataFormat,AudioFreq,AudioFreqCustom
I2S2.Instance=SPI$Index
I2S2.RealAudioFreq=32.0 KHz
I2S3.AudioFreq=AudioFreqCustomValue
I2S3.AudioFreqCustom=32000
I2S3.DataFormat=I2S_DATAFORMAT_32B
I2S3.ErrorAudioFreq=0.0 %
I2S3.IPParameters=Instance,RealAudioFreq,ErrorAudioFreq,DataFormat,AudioFreq,AudioFreqCustom
I2S3.Instance=SPI$Index
I2S3.RealAudioFreq=32.0 KHz
KeepUserPlacement=false
MMTAppReg1.MEMORYMAP.AP=RW_priv_only
MMTAppReg1.MEMORYMAP.AppRegionName=RAM
MMTAppReg1.MEMORYMAP.ContextName=CortexM33
MMTAppReg1.MEMORYMAP.CoreName=ARM Cortex-M33
MMTAppReg1.MEMORYMAP.DefaultDataRegion=true
MMTAppReg1.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,DefaultDataRegion,ContextName,Name,AP
MMTAppReg1.MEMORYMAP.Name=RAM
MMTAppReg1.MEMORYMAP.Size=278528
MMTAppReg1.MEMORYMAP.StartAddress=0x20000000
MMTAppReg2.MEMORYMAP.AppRegionName=RAM Reserved Alias Region
MMTAppReg2.MEMORYMAP.CoreName=ARM Cortex-M33
MMTAppReg2.MEMORYMAP.DefaultDataRegion=false
MMTAppReg2.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,DefaultDataRegion,ReservedRegion,Name
MMTAppReg2.MEMORYMAP.Name=RAM Reserved Alias Region
MMTAppReg2.MEMORYMAP.ReservedRegion=true
MMTAppReg2.MEMORYMAP.Size=278528
MMTAppReg2.MEMORYMAP.StartAddress=0x0A000000
MMTAppReg3.MEMORYMAP.AP=RO_priv_only
MMTAppReg3.MEMORYMAP.AppRegionName=FLASH
MMTAppReg3.MEMORYMAP.Cacheability=WTRA
MMTAppReg3.MEMORYMAP.ContextName=CortexM33
MMTAppReg3.MEMORYMAP.CoreName=ARM Cortex-M33
MMTAppReg3.MEMORYMAP.DefaultCodeRegion=true
MMTAppReg3.MEMORYMAP.DefaultDataRegion=false
MMTAppReg3.MEMORYMAP.IPParameters=StartAddress,Size,CoreName,DefaultDataRegion,MemType,ContextName,Name,AP,Cacheability,DefaultCodeRegion
MMTAppReg3.MEMORYMAP.MemType=ROM
MMTAppReg3.MEMORYMAP.Name=FLASH
MMTAppReg3.MEMORYMAP.Size=524288
MMTAppReg3.MEMORYMAP.StartAddress=0x08000000
MMTAppRegionsCount=3
MMTConfigApplied=false
MMTSectionSuffix=
Mcu.CPN=STM32H533RET6
Mcu.ContextProject=TrustZoneDisabled
Mcu.Family=STM32H5
Mcu.IP0=BOOTPATH
Mcu.IP1=CORTEX_M33_NS
Mcu.IP10=NVIC
Mcu.IP11=PWR
Mcu.IP12=RCC
Mcu.IP13=SYS
Mcu.IP14=TIM2
Mcu.IP15=TIM5
Mcu.IP16=UART5
Mcu.IP17=USART2
Mcu.IP18=USART3
Mcu.IP2=DEBUG
Mcu.IP3=GPDMA1
Mcu.IP4=GPDMA2
Mcu.IP5=I2C1
Mcu.IP6=I2S2
Mcu.IP7=I2S3
Mcu.IP8=ICACHE
Mcu.IP9=MEMORYMAP
Mcu.IPNb=19
Mcu.Name=STM32H533RETx
Mcu.Package=LQFP64
Mcu.Pin0=PC14-OSC32_IN(OSC32_IN)
Mcu.Pin1=PC15-OSC32_OUT(OSC32_OUT)
Mcu.Pin10=PB10
Mcu.Pin11=PB12
Mcu.Pin12=PB13
Mcu.Pin13=PB14
Mcu.Pin14=PB15
Mcu.Pin15=PC6
Mcu.Pin16=PC7
Mcu.Pin17=PA13(JTMS/SWDIO)
Mcu.Pin18=PA14(JTCK/SWCLK)
Mcu.Pin19=PA15(JTDI)
Mcu.Pin2=PH0-OSC_IN(PH0)
Mcu.Pin20=PC10
Mcu.Pin21=PC11
Mcu.Pin22=PC12
Mcu.Pin23=PD2
Mcu.Pin24=PB4(NJTRST)
Mcu.Pin25=PB5
Mcu.Pin26=PB6
Mcu.Pin27=PB7
Mcu.Pin28=PB8
Mcu.Pin29=VP_CORTEX_M33_NS_VS_Hclk
Mcu.Pin3=PH1-OSC_OUT(PH1)
Mcu.Pin30=VP_GPDMA1_VS_GPDMACH0
Mcu.Pin31=VP_GPDMA1_VS_GPDMACH1
Mcu.Pin32=VP_GPDMA1_VS_GPDMACH2
Mcu.Pin33=VP_GPDMA1_VS_GPDMACH3
Mcu.Pin34=VP_GPDMA2_VS_GPDMACH0
Mcu.Pin35=VP_GPDMA2_VS_GPDMACH1
Mcu.Pin36=VP_GPDMA2_VS_GPDMACH2
Mcu.Pin37=VP_GPDMA2_VS_GPDMACH3
Mcu.Pin38=VP_ICACHE_VS_ICACHE
Mcu.Pin39=VP_PWR_VS_SECSignals
Mcu.Pin4=PC2
Mcu.Pin40=VP_PWR_VS_LPOM
Mcu.Pin41=VP_SYS_VS_Systick
Mcu.Pin42=VP_TIM2_VS_ClockSourceINT
Mcu.Pin43=VP_TIM5_VS_ClockSourceINT
Mcu.Pin44=VP_BOOTPATH_VS_BOOTPATH
Mcu.Pin45=VP_MEMORYMAP_VS_MEMORYMAP
Mcu.Pin5=PA0
Mcu.Pin6=PA1
Mcu.Pin7=PA2
Mcu.Pin8=PA3
Mcu.Pin9=PB1
Mcu.PinsNb=46
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32H533RETx
MxCube.Version=6.16.1
MxDb.Version=DB.6.0.161
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.ForceEnableDMAVector=false
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:false\:false\:false
NVIC.UART5_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
PA0.GPIOParameters=PinState,GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PA0.GPIO_Label=CODEC_RST
PA0.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PA0.GPIO_PuPd=GPIO_PULLUP
PA0.Locked=true
PA0.PinState=GPIO_PIN_SET
PA0.Signal=GPIO_Output
PA1.GPIOParameters=GPIO_Speed
PA1.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA1.Mode=Hardware Flow Control (RS485)
PA1.Signal=USART2_DE
PA13(JTMS/SWDIO).Mode=Serial_Wire
PA13(JTMS/SWDIO).Signal=DEBUG_JTMS-SWDIO
PA14(JTCK/SWCLK).Mode=Serial_Wire
PA14(JTCK/SWCLK).Signal=DEBUG_JTCK-SWCLK
PA15(JTDI).GPIOParameters=GPIO_Speed
PA15(JTDI).GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PA15(JTDI).Locked=true
PA15(JTDI).Mode=Full_Duplex_Master
PA15(JTDI).Signal=I2S3_WS
PA2.GPIOParameters=GPIO_Speed
PA2.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.GPIOParameters=GPIO_Speed,PinAttribute
PA3.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA3.Mode=Asynchronous
PA3.PinAttribute=Free
PA3.Signal=USART2_RX
PB1.GPIOParameters=GPIO_Speed,PinAttribute
PB1.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PB1.Locked=true
PB1.Mode=Asynchronous
PB1.PinAttribute=Free
PB1.Signal=USART3_RX
PB10.GPIOParameters=GPIO_Speed,PinAttribute
PB10.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PB10.Mode=Asynchronous
PB10.PinAttribute=Free
PB10.Signal=USART3_TX
PB12.GPIOParameters=GPIO_Speed,PinAttribute
PB12.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PB12.Mode=Full_Duplex_Master
PB12.PinAttribute=Free
PB12.Signal=I2S2_WS
PB13.GPIOParameters=GPIO_Speed,PinAttribute
PB13.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PB13.Locked=true
PB13.Mode=Full_Duplex_Master
PB13.PinAttribute=Free
PB13.Signal=I2S2_CK
PB14.GPIOParameters=GPIO_Speed,PinAttribute
PB14.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PB14.Mode=Hardware Flow Control (RS485)
PB14.PinAttribute=Free
PB14.Signal=USART3_DE
PB15.GPIOParameters=GPIO_Speed,PinAttribute
PB15.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PB15.Locked=true
PB15.Mode=Full_Duplex_Master
PB15.PinAttribute=Free
PB15.Signal=I2S2_SDO
PB4(NJTRST).GPIOParameters=GPIO_Speed
PB4(NJTRST).GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PB4(NJTRST).Locked=true
PB4(NJTRST).Mode=Full_Duplex_Master
PB4(NJTRST).Signal=I2S3_SDI
PB5.GPIOParameters=GPIO_Speed
PB5.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PB5.Locked=true
PB5.Mode=Full_Duplex_Master
PB5.Signal=I2S3_SDO
PB6.GPIOParameters=PinAttribute
PB6.Mode=I2C
PB6.PinAttribute=Free
PB6.Signal=I2C1_SCL
PB7.GPIOParameters=PinAttribute
PB7.Mode=I2C
PB7.PinAttribute=Free
PB7.Signal=I2C1_SDA
PB8.GPIOParameters=GPIO_Label,PinAttribute
PB8.GPIO_Label=SHR_DOUT_DISP
PB8.Locked=true
PB8.PinAttribute=Free
PB8.Signal=GPIO_Output
PC10.GPIOParameters=GPIO_Speed
PC10.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PC10.Mode=Full_Duplex_Master
PC10.Signal=I2S3_CK
PC11.GPIOParameters=PinState,GPIO_Label,PinAttribute
PC11.GPIO_Label=LD2
PC11.Locked=true
PC11.PinAttribute=Free
PC11.PinState=GPIO_PIN_SET
PC11.Signal=GPIO_Output
PC12.GPIOParameters=PinAttribute
PC12.Locked=true
PC12.Mode=Asynchronous
PC12.PinAttribute=Free
PC12.Signal=UART5_TX
PC14-OSC32_IN(OSC32_IN).GPIOParameters=GPIO_Label,PinAttribute
PC14-OSC32_IN(OSC32_IN).GPIO_Label=SHR_CLK
PC14-OSC32_IN(OSC32_IN).Locked=true
PC14-OSC32_IN(OSC32_IN).PinAttribute=Free
PC14-OSC32_IN(OSC32_IN).Signal=GPIO_Output
PC15-OSC32_OUT(OSC32_OUT).GPIOParameters=GPIO_Label,PinAttribute
PC15-OSC32_OUT(OSC32_OUT).GPIO_Label=SHR_STR
PC15-OSC32_OUT(OSC32_OUT).Locked=true
PC15-OSC32_OUT(OSC32_OUT).PinAttribute=Free
PC15-OSC32_OUT(OSC32_OUT).Signal=GPIO_Output
PC2.GPIOParameters=GPIO_Speed
PC2.GPIO_Speed=GPIO_SPEED_FREQ_MEDIUM
PC2.Mode=Full_Duplex_Master
PC2.Signal=I2S2_SDI
PC6.GPIOParameters=GPIO_Speed
PC6.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PC6.Mode=Master_Clock_Activated
PC6.Signal=I2S2_MCK
PC7.GPIOParameters=GPIO_Speed
PC7.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PC7.Mode=Master_Clock_Activated
PC7.Signal=I2S3_MCK
PCC.Checker=false
PCC.Line=STM32H5x3
PCC.MCU=STM32H533RETx
PCC.PartNumber=STM32H533RETx
PCC.Series=STM32H5
PCC.Temperature=25
PCC.Vdd=3.0
PD2.GPIOParameters=PinAttribute
PD2.Locked=true
PD2.Mode=Asynchronous
PD2.PinAttribute=Free
PD2.Signal=UART5_RX
PH0-OSC_IN(PH0).Mode=HSE-External-Oscillator
PH0-OSC_IN(PH0).Signal=RCC_OSC_IN
PH1-OSC_OUT(PH1).Mode=HSE-External-Oscillator
PH1-OSC_OUT(PH1).Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerLinker=GCC
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32H533RETx
ProjectManager.FirmwarePackage=STM32Cube FW_H5 V1.5.1
ProjectManager.FreePins=false
ProjectManager.FreePinsContext=
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=DigitalAudioH533.ioc
ProjectManager.ProjectName=DigitalAudioH533
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-LL-false,2-MX_GPIO_Init-GPIO-false-LL-true,3-MX_GPDMA1_Init-GPDMA1-false-LL-true,4-MX_GPDMA2_Init-GPDMA2-false-LL-true,5-MX_ICACHE_Init-ICACHE-false-LL-true,6-MX_TIM5_Init-TIM5-false-LL-true,7-MX_TIM2_Init-TIM2-false-LL-true,8-MX_USART3_UART_Init-USART3-false-LL-true,9-MX_UART5_Init-UART5-false-LL-true,10-MX_USART2_UART_Init-USART2-false-LL-true,11-MX_I2S2_Init-I2S2-false-LL-true,12-MX_I2C1_Init-I2C1-false-LL-true,13-MX_I2S3_Init-I2S3-false-LL-true,0-MX_CORTEX_M33_NS_Init-CORTEX_M33_NS-false-LL-true,0-MX_PWR_Init-PWR-false-LL-true
RCC.ADCFreq_Value=80000000
RCC.AHBFreq_Value=80000000
RCC.APB1Freq_Value=80000000
RCC.APB1TimFreq_Value=80000000
RCC.APB2Freq_Value=80000000
RCC.APB2TimFreq_Value=80000000
RCC.APB3Freq_Value=80000000
RCC.CKPERFreq_Value=16000000
RCC.CKPERSourceSelection=RCC_CLKPSOURCE_HSE
RCC.CRSFreq_Value=48000000
RCC.CSI_VALUE=4000000
RCC.CortexFreq_Value=80000000
RCC.DACFreq_Value=32768
RCC.EPOD_VALUE=16000000
RCC.FCLKCortexFreq_Value=80000000
RCC.FDCANFreq_Value=16000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=80000000
RCC.HSE_VALUE=16000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=64000000
RCC.I2C1CLockSelection=RCC_I2C1CLKSOURCE_PLL3R
RCC.I2C1Freq_Value=32000000
RCC.I2C2Freq_Value=80000000
RCC.I2C3Freq_Value=80000000
RCC.I3C1Freq_Value=80000000
RCC.I3C2Freq_Value=80000000
RCC.IPParameters=ADCFreq_Value,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,APB3Freq_Value,CKPERFreq_Value,CKPERSourceSelection,CRSFreq_Value,CSI_VALUE,CortexFreq_Value,DACFreq_Value,EPOD_VALUE,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1CLockSelection,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I3C1Freq_Value,I3C2Freq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_VALUE,LSIRC_VALUE,MCO1PinFreq_Value,MCO2PinFreq_Value,OCTOSPIMFreq_Value,PLL1P,PLL1Q,PLL2M,PLL2N,PLL2P,PLL2PoutputFreq_Value,PLL2Q,PLL2QoutputFreq_Value,PLL2RoutputFreq_Value,PLL2Source,PLL3N,PLL3PoutputFreq_Value,PLL3Q,PLL3QoutputFreq_Value,PLL3R,PLL3RoutputFreq_Value,PLL3Source,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLSourceVirtual,PWRFreq_Value,RNGFreq_Value,SDMMC1Freq_Value,SPI1Freq_Value,SPI2CLockSelection,SPI2Freq_Value,SPI3CLockSelection,SPI3Freq_Value,SPI4Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5CLockSelection,UART5Freq_Value,UCPD1outputFreq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBFreq_Value,VCOInput2Freq_Value,VCOInput3Freq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOPLL2OutputFreq_Value,VCOPLL3OutputFreq_Value
RCC.LPTIM1Freq_Value=80000000
RCC.LPTIM2Freq_Value=80000000
RCC.LPUART1Freq_Value=80000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_VALUE=32768
RCC.LSIRC_VALUE=32000
RCC.MCO1PinFreq_Value=32000000
RCC.MCO2PinFreq_Value=80000000
RCC.OCTOSPIMFreq_Value=80000000
RCC.PLL1P=4
RCC.PLL1Q=10
RCC.PLL2M=10
RCC.PLL2N=256
RCC.PLL2P=10
RCC.PLL2PoutputFreq_Value=40960000
RCC.PLL2Q=10
RCC.PLL2QoutputFreq_Value=40960000
RCC.PLL2RoutputFreq_Value=204800000
RCC.PLL2Source=RCC_PLL2_SOURCE_HSE
RCC.PLL3N=8
RCC.PLL3PoutputFreq_Value=64000000
RCC.PLL3Q=4
RCC.PLL3QoutputFreq_Value=32000000
RCC.PLL3R=4
RCC.PLL3RoutputFreq_Value=32000000
RCC.PLL3Source=RCC_PLL3_SOURCE_HSE
RCC.PLLN=20
RCC.PLLPoutputFreq_Value=80000000
RCC.PLLQoutputFreq_Value=32000000
RCC.PLLSourceVirtual=RCC_PLL1_SOURCE_HSE
RCC.PWRFreq_Value=80000000
RCC.RNGFreq_Value=48000000
RCC.SDMMC1Freq_Value=32000000
RCC.SPI1Freq_Value=32000000
RCC.SPI2CLockSelection=RCC_SPI2CLKSOURCE_PLL2P
RCC.SPI2Freq_Value=40960000
RCC.SPI3CLockSelection=RCC_SPI3CLKSOURCE_PLL2P
RCC.SPI3Freq_Value=40960000
RCC.SPI4Freq_Value=80000000
RCC.SYSCLKFreq_VALUE=80000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=80000000
RCC.UART5CLockSelection=RCC_UART5CLKSOURCE_PLL3Q
RCC.UART5Freq_Value=32000000
RCC.UCPD1outputFreq_Value=8000000
RCC.USART1Freq_Value=80000000
RCC.USART2Freq_Value=80000000
RCC.USART3Freq_Value=80000000
RCC.USART6Freq_Value=80000000
RCC.USBFreq_Value=48000000
RCC.VCOInput2Freq_Value=1600000
RCC.VCOInput3Freq_Value=16000000
RCC.VCOInputFreq_Value=16000000
RCC.VCOOutputFreq_Value=320000000
RCC.VCOPLL2OutputFreq_Value=409600000
RCC.VCOPLL3OutputFreq_Value=128000000
TIM2.IPParameters=Prescaler
TIM2.Prescaler=39999
TIM5.IPParameters=Prescaler
TIM5.Prescaler=79
USART2.BaudRate=5000000
USART2.IPParameters=VirtualMode-Asynchronous,VirtualMode-Hardware Flow Control (RS485),BaudRate
USART2.VirtualMode-Asynchronous=VM_ASYNC
USART2.VirtualMode-Hardware\ Flow\ Control\ (RS485)=VM_ASYNC
USART3.BaudRate=5000000
USART3.IPParameters=VirtualMode-Asynchronous,VirtualMode-Hardware Flow Control (RS485),BaudRate,OverSampling
USART3.OverSampling=UART_OVERSAMPLING_16
USART3.VirtualMode-Asynchronous=VM_ASYNC
USART3.VirtualMode-Hardware\ Flow\ Control\ (RS485)=VM_ASYNC
VP_BOOTPATH_VS_BOOTPATH.Mode=BP_Activate
VP_BOOTPATH_VS_BOOTPATH.Signal=BOOTPATH_VS_BOOTPATH
VP_CORTEX_M33_NS_VS_Hclk.Mode=Hclk_Mode
VP_CORTEX_M33_NS_VS_Hclk.Signal=CORTEX_M33_NS_VS_Hclk
VP_GPDMA1_VS_GPDMACH0.Mode=SIMPLEREQUEST_GPDMACH0
VP_GPDMA1_VS_GPDMACH0.Signal=GPDMA1_VS_GPDMACH0
VP_GPDMA1_VS_GPDMACH1.Mode=SIMPLEREQUEST_GPDMACH1
VP_GPDMA1_VS_GPDMACH1.Signal=GPDMA1_VS_GPDMACH1
VP_GPDMA1_VS_GPDMACH2.Mode=SIMPLEREQUEST_GPDMACH2
VP_GPDMA1_VS_GPDMACH2.Signal=GPDMA1_VS_GPDMACH2
VP_GPDMA1_VS_GPDMACH3.Mode=SIMPLEREQUEST_GPDMACH3
VP_GPDMA1_VS_GPDMACH3.Signal=GPDMA1_VS_GPDMACH3
VP_GPDMA2_VS_GPDMACH0.Mode=SIMPLEREQUEST_GPDMACH0
VP_GPDMA2_VS_GPDMACH0.Signal=GPDMA2_VS_GPDMACH0
VP_GPDMA2_VS_GPDMACH1.Mode=SIMPLEREQUEST_GPDMACH1
VP_GPDMA2_VS_GPDMACH1.Signal=GPDMA2_VS_GPDMACH1
VP_GPDMA2_VS_GPDMACH2.Mode=SIMPLEREQUEST_GPDMACH2
VP_GPDMA2_VS_GPDMACH2.Signal=GPDMA2_VS_GPDMACH2
VP_GPDMA2_VS_GPDMACH3.Mode=SIMPLEREQUEST_GPDMACH3
VP_GPDMA2_VS_GPDMACH3.Signal=GPDMA2_VS_GPDMACH3
VP_ICACHE_VS_ICACHE.Mode=DefaultMode
VP_ICACHE_VS_ICACHE.Signal=ICACHE_VS_ICACHE
VP_MEMORYMAP_VS_MEMORYMAP.Mode=CurAppReg
VP_MEMORYMAP_VS_MEMORYMAP.Signal=MEMORYMAP_VS_MEMORYMAP
VP_PWR_VS_LPOM.Mode=PowerOptimisation
VP_PWR_VS_LPOM.Signal=PWR_VS_LPOM
VP_PWR_VS_SECSignals.Mode=Security/Privilege
VP_PWR_VS_SECSignals.Signal=PWR_VS_SECSignals
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM2_VS_ClockSourceINT.Mode=Internal
VP_TIM2_VS_ClockSourceINT.Signal=TIM2_VS_ClockSourceINT
VP_TIM5_VS_ClockSourceINT.Mode=Internal
VP_TIM5_VS_ClockSourceINT.Signal=TIM5_VS_ClockSourceINT
board=custom
